Up-to-date list of accepted command line parameters
===================================================

Usage:
atari800 [options] [disk1 ... disk8]

where:
disk1 ... disk8 are file names of the disk images mounted to Atari drives 1-8
(the first file is mounted to the drive 1, next one to the drive 2, etc.).
Supported types of disk images are: ATR, XFD and DCM. If the emulator has been
compiled with ZLIB support, additionally ATR.GZ and XFD.GZ are supported.

Options
-------

-help                 Display list of options and terminate
-v                    Display version number and terminate
-verbose              Display framerate when exiting

-configure            Update configuration file (this is default
                      if the configuration file has not been found)
-config <filename>    Use specified configuration file instead of default
-osa_rom <filename>   Use specified OS/A ROM image
-osb_rom <filename>   Use specified OS/B ROM image
-xlxe_rom <filename>  Use specified XL/XE OS ROM image
-5200_rom <filename>  Use specified 5200 OS ROM image
-basic_rom <filename> Use specified Atari BASIC ROM image

-atari                Emulate Atari 800
-xl                   Emulate Atari 800 XL
-xe                   Emulate Atari 130 XE
-320xe                Emulate Atari 320 XE (Compy Shop)
-rambo                Emulate Atari 320 XE (Rambo)
-5200                 Emulate Atari 5200
-emuos                Use EmuOS

-a                    Use OS/A for Atari 800
-b                    Use OS/B for Atari 800
-c                    Enable RAM between 0xc000 and 0xcfff in Atari 800

-pal                  Emulate PAL TV mode
-ntsc                 Emulate NTSC TV mode

-nobasic              Turn off Atari BASIC ROM
-basic                Turn on Atari BASIC ROM

-cart <filename>      Insert cartridge (CART or raw format)

-run <filename>       Run Atari executable file (EXE, COM, XEX)

-tape <filename>      Attach cassette image (CAS format or raw file)
-boottape <filename>  Attach cassette image and boot it

-nopatch              Don't patch SIO routine in OS
-nopatchall           Don't patch OS at all, H: and P: devices won't work
-H1 <path>            Set path for H1: device
-H2 <path>            Set path for H2: device
-H3 <path>            Set path for H3: device
-H4 <path>            Set path for H4: device
-hdreadonly <onoff>   Enable (1) or disable (0) read-only mode for H: device
-devbug               Put debugging messages for H: and P: devices in log file

-rtime <onoff>        Enable (1) or disable (0) R-Time 8 emulation

-mouse off            Do not use mouse
-mouse pad            Emulate paddles
-mouse touch          Emulate Atari Touch Tablet
-mouse koala          Emulate Koala Pad
-mouse pen            Emulate Light Pen
-mouse gun            Emulate Light Gun
-mouse amiga          Emulate Amiga mouse
-mouse st             Emulate Atari ST mouse
-mouse trak           Emulate Atari Trak-Ball
-mouse joy            Emulate joystick using mouse
-mouseport <num>      Set mouse port 1-4 (default 1)
-mousespeed <num>     Set mouse speed 1-9 (default 3)

-refresh <rate>       Set screen refresh rate
-artif <mode>         Set artifacting mode 0-4 (0 = disable)
-palette <filename>   Read Atari colors from ACT file
-black <num>          Set black level 0-255
-while <num>          Set white level 0-255
-colors <num>         Set color intensity
-colshift <num>       Set color shift
-realpal              Use palette created by Zdenek Eisenhammer
-oldpal               Use old Atari800 palette
-foxpal               Use palette created by Piotr Fusik

-sound                Enable sound
-nosound              Disable sound
-dsprate <freq>       Set mixing frequency (Hz)
-snddelay <time>      Set sound delay (milliseconds)

Curses version options
----------------------
-left                 Use columns 0 to 39
-central              Use columns 20 to 59
-right                Use columns 40 to 79
-wide1                Use columns 0 to 79 (spaces between characters)
-wide2                Use columns 0 to 79 (as above but normal/reverse spaces)

Falcon version options
----------------------

-interlace <x>        Generate Falcon screen only every x frame
-videl                Direct VIDEL programming (Falcon/VGA only)
-double               Double the screen size on NOVA
-delta                Delta screen output (differences only)

-joyswap              Swap joysticks

SVGALIB version options
-----------------------

-interlace            Generate screen with interlace

DOS/VGA version options
-----------------------

-interlace            Generate screen with interlace
-video <mode>         0=320x200, 1=320x240, 2=320x480 interlaced with black
                      lines, 3=320x480 interlaced with darker lines
-novesa               Do not use VESA 2 video modes
-vretrace             Use vertical retrace control

-LPTjoy1              Read joystick connected to LPT1
-LPTjoy2              Read joystick connected to LPT2
-LPTjoy3              Read joystick connected to LPT3
-joyswap              Swap joysticks

-keyboard 0           PC keyboard layout
-keyboard 1           Atari keyboard layout

X11 options
-----------

-small                Single size window
-large                Double size window
-huge                 Triple size window
-clip_x <n>           Left offset for clipping
-clip_y <n>           Top offset for clipping
-clip_width           Width of the clipping area
-clip_height          Height of the clipping area
-private_cmap         Use private colormap

-fps                  Show framerate
-sio                  Show SIO monitor
-x11bug               Enable debug code in atari_x11.c

-keypad               Keypad mode

SDL version options
-------------------

-nojoystick 	      joysticks will not be initialized
-joy0 </dev/lp0>      define the device for LPTjoy
-joy1 </dev/lp1>      --""-- only when LPTjoy support compiled in
-rotate90             useful for devices with 240x320 screen (hanhelds)
-width x              set mode width
-height y             set mode height
-bpp b                set mode bits per pixel
-fullscreen           start in fullscreen mode
-windowed             start in windowed mode

Keyboard + Joystick & Paddle Controllers
========================================

Unlike PC Xformer, I have not tried to emulate the exact keyboard layout,
instead, I have tried to make your native keyboard work as normal.

Note: The function keys will eventually be changed to a more logical
      order.

X11 Keyboard + Joystick & Paddle Controllers
============================================

F1	Built in User Interface
F2	Option
F3	Select
F4	Start
F5	Warm Reset
Shft+F5	Cold Reset
F6	Toggle RAM/ROM between 0x8000 and 0xbfff (PIL Mode)
F7	Break Key
F8	---
F9	Exit Emulator
F10	---
F11	Vertical Positioning: Scroll Screen Downwards
F12	Vertical Positioning: Scroll Screen Upwards

ALT	Atari Key (Either ALT Key will work)

Joystick 0 is operated by the mouse position relative to the center of the
screen. The mouse button acts as the trigger.

Paddle 0 is operated by moving the mouse pointer across the window.

SVGALIB Keyboard + Joystick & Paddle Controllers
================================================

F1	Built in User Interface
F2	Option
F3	Select
F4	Start
F5	Warm Reset
Shft+F5	Cold Reset
F6	Toggle RAM/ROM between 0x8000 and 0xbfff (PIL Mode)
F7	Break Key
F8	Enter monitor
F9	Exit Emulator
F10	Save Screenshot (+Shift=interlaced screenshot)
F11	Joystick Autofire On/Off
F12	---

`	This character replaces the CAPS lock key because I have not
	found a way of detecting it. A future solution maybe to
	automatically issue a CAPS lock key when a transition is
	made between lower and upper case keys. i.e. If svgalib
	return 'a' followed by 'A' it could send 'a' 'CAPS' 'A' to
	the Atari.

The CTRL+SHIFT keyboard combinations are implemented using the left
ALT key.

Joystick 0 is operated by the numeric keypad (make sure that the numeric
keypad has been enabled).

	7 8 9
	 \|/
	4 5 6
	 /|\
	1 2 3

	And 0 is the fire key.

At the moment it is not possible to use a Paddle with the SVGALIB version.

CURSES Keyboard + Joystick & Paddle Controllers
===============================================

F1	Built in User Interface
F2	Option
F3	Select
F4	Start
F5	Warm Reset
F6	Toggle RAM/ROM between 0x8000 and 0xbfff (PIL Mode)
F7	Break Key
F8	Cold Reset
F9	Exit Emulator
F10	---
F11	---
F12	---

Some control have special meaning within curses and should not be used.

	Avoid Control + C, J, M, Q, S and Z

The remaining control characters can be typed. Control characters are
displayed on the screen with the associated upper case character in bold.

No Joystick or Paddle support in this version.

AMIGA Keyboard + Joystick & Paddle Controllers
==============================================

Please look into the supplied Atari800.guide

BASIC Keyboard + Joystick & Paddle Controllers
==============================================

No Frills text. Upper and Lower case letters, 0-9, !"$% etc.
No Reset, Option, Select, Start, etc.
No Joystick or Paddle support in this version.

DOS VGA Keyboard + Joystick & Paddle Controllers
================================================

F1	Built in User Interface
F2	Option Key
F3	Select Key
F4	Start Key
F5	Warm Reset
Shft+F5	Cold Reset
F6	PIL Mode (Atari800) / Help Key (XL/XE)
F7	Switch between Emulated joysticks mode and Normal keyboard
F8	Enter monitor
F9	EXIT Emulator
F10	Save Screenshot (+Shift=interlaced screenshot)

Control-C terminates the program; to type Control-c, type ALT-c instead.
` is used as the Atari-Invers key

Joysticks can be either real one connected to game port, or old 8-bit
digital CX-40 joysticks connected to parallel port or keyboard joysticks
(try out JOYCFG.EXE).
 
At the moment it is not possible to use a Paddle with this version.

Falcon Keyboard + Joystick & Paddle Controllers
===============================================

F1	Built in User Interface
F2	Option
F3	Select
F4	Start
F5	Warm Reset
Shft+F5	Cold Reset
F6	Toggle RAM/ROM between 0x8000 and 0xbfff (PIL Mode)
F7	Break Key
F8	Enter monitor
F9	EXIT Emulator
Help	HELP key (800XL/130XE)

Joystick 0 is operated by the numeric keypad (make sure that the numeric
keypad has been enabled).
 
        7 8 9
         \|/
        4 5 6
         /|\
        1 2 3
 
        And 0 is the fire key.
 
At the moment it is not possible to use a Paddle with this version.

SDL port keys and options
=========================

-joy0 <pathname>      Select LPTjoy0 device; ex.:
                      $ atari800 -joy0 /dev/lp0 ...
-joy1 <pathname>      Select LPTjoy1 device

LALT+f - switching FULLSCREEN (probably doesn't work in Windows)
LALT+g - switching WIDTH_MODE (so you can set 320x240)
LALT+b - switching BLACK-AND-WHITE (feel to power of BW monitor!)
LALT+j - swapping _keyboard_emulated_ joysticks
LALT+e - switching bpp (for debug only, will be removed soon)

To redefine keys for joystick emulation you must modify SDL_TRIG_* and
SDL_JOY_* in atari_sdl.c, then recompile Atari800. In source you can also turn
off sound or change defaults (FULLSCREEN, BW, SWAP_JOYSTICKS, WIDTH_MODE).

